|  |  |  |
| --- | --- | --- |
| **DESCRIPTION**   * Uniform hollow-cone wide angle spray pattern. * Atomisation becomes finer at higher pressure and wider spray angles. * Swirl chamber designed with counterbore for improved spray quality. * Available in Nylon/PP only * Available in 1⁄4” and 3⁄4” Male | |  |
| **SPECIFICATIONS** |  | |
| |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | |  | Thread | | eq. orifice [mm] | | Flow Rate (lpm) @ Pressure (Bar) | | | | | | | Spray Angle (°)  @ 3 pressure (bar) | | TYPE | 1/4" | 3/4” | Outlet | Inlet | 1 | 2 | 3 | 4 | 5 | 6 | 7 |  | | 2 | 🗹 | - | 1,6 | 1,6 | 0,45 | 0,64 | 0,79 | 0,91 | 1,0 | 1,1 | 1,2 | 115 | | 4 | 🗹 | - | 2,5 | 2,1 | 0,92 | 1,3 | 1,6 | 1,8 | 2,0 | 2,2 | 2,4 | 115 | | 5 | 🗹 | - | 2,5 | 2,6 | 1,1 | 1,6 | 2,0 | 2,3 | 2,5 | 2,8 | 3,0 | 110 | | 6 | 🗹 | - | 2,5 | 3,1 | 1,3 | 1,9 | 2,4 | 2,7 | 3,1 | 3,4 | 3,6 | 110 | | 10 | 🗹 | - | 3,5 | 3,5 | 2,3 | 3,2 | 3,9 | 4,6 | 5,1 | 5,6 | 6,0 | 110 | | 15 | 🗹 | - | 4,0 | 3,9 | 3,4 | 4,8 | 5,9 | 6,8 | 7,6 | 8,4 | 9,0 | 110 | | 20 | 🗹 | - | 5,6 | 3,9 | 4,5 | 6,4 | 7,9 | 9,1 | 10,2 | 11,2 | 12,1 | 110 | | 25 | - | 🗹 | 8,3 | 3,8 | 4,56 | 6,45 | 7,9 | 9,12 | 10,2 | 11,2 | 12,1 | 140 | | 30 | - | 🗹 | 9,3 | 4,9 | 6,84 | 9,67 | 11,8 | 13,7 | 15,3 | 16,7 | 18,1 | 140 | | 40 | - | 🗹 | 9,3 | 6,2 | 9,12 | 12,9 | 15,8 | 18,2 | 20,4 | 22,4 | 24,1 | 140 | | 60 | - | 🗹 | 10,3 | 7,9 | 13,7 | 19,3 | 23,7 | 27,4 | 30,6 | 33,4 | 36,2 | 140 | | 80 | - | 🗹 | 15,9 | 7,1 | 18,2 | 25,8 | 31,5 | 36,5 | 40,8 | 44,6 | 48,3 | 140 | | 100 | - | 🗹 | 15,9 | 8,2 | 22,8 | 32,2 | 39,5 | 45,6 | 51,0 | 55,8 | 60,3 | 140 | | 120 | - | 🗹 | 17,4 | 8,6 | 27,3 | 38,7 | 47,4 | 54,7 | 61,2 | 67,0 | 72,4 | 140 | | 160 | - | 🗹 | 20,6 | 9,6 | 36,5 | 51,6 | 63,2 | 73,0 | 81,6 | 89,4 | 96,5 | 140 | | 200 | - | 🗹 | 20,6 | 10,7 | 45,6 | 64,5 | 79,0 | 91,2 | 102 | 112 | 121 | 140 | | 240 | - | 🗹 | 20,6 | 12,1 | 54,7 | 77,4 | 94,7 | 109 | 122 | 134 | 145 | 140 | | | |
| **DIMENSIONS** |  | |
|  | |  |  |  |  | | --- | --- | --- | --- | |  | **Dimensions** | | | | Thread | **A** | **B(Dia)** | **C** | | (mm) | | | | 1/4" | 33.3 | 19.1 | 24.6 | | 3/4" | 69.1 | 40.0 | 47.2 | | |
| **HOW TO ORDER**  TEXTRA 1/4" WRW Type Material  **TEXTRA 1/4" WRW 60 Nylon** | | |